**LISTING LABEL ORDER FORM**

Minimum order: USD 50.00 for 500 labels, additional rolls of 250 are USD 25.00 per roll.

Dimensions: 3.6 inches (9.144 cm) wide by 1.2 inches (3.048 cm) high

**Example:**   

|  |  |
| --- | --- |
| **Bill To** | **Ship To,** *if different from Bill to* |
| Company: [Enter Company Name]Attention Name: [Enter Name]Address: [Enter Co Address]City: [Enter Co City] State/Province: [Enter State/Province] Zip/Postal Code: [Enter Zip/Postal Code] Country: [Enter Country] PO #: Enter text. | Manufacturing Company: [Enter Company Name]Attention Name: [Enter Name]Address: [Enter Co Address]City: [Enter Co City] State/Province: [Enter State/Province] Zip/Postal Code: [Enter Zip/Postal Code] Country: [Enter Country] |
| **Order Contact** | **Shipping Account**  |
| Full Name: Enter text. Title: Enter text.Email: Enter text.Phone: Enter text. | DHL Account: Enter text. FedEx Account: Enter text.UPS: Enter text. [ ]  Regular [ ]  Expedite *Shipping will default to regular if not selected.* |
| **Engineering Contact** | **Marketing Contact**  |
| Full Name: Enter text. Title: Enter text.Email: Enter text.Phone: Enter text. | Full Name: Enter text. Title: Enter text.Email: Enter text.Phone: Enter text. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Label** | **Description** | **Your part#**  | **# of Rolls****Min. 2** | **Amount****Min. USD 50** |
| CT-AMCA 540 | Cycle Tested per AMCA 540 | [enter]  | [enter]  | [enter]  |
| HVRR-FC | High Velocity Rain Resistant with Blades Fully Closed -550 | [enter]  | [enter]  | [enter]  |
| HVRR & IR–FC-D | High Velocity Rain Resistant with Blades Fully Closed & Impact Resistant Louver - Basic Protection Level D | [enter]  | [enter]  | [enter]  |
| HVRR & IR–FC-E | High Velocity Rain Resistant with Blades Fully Closed & Impact Resistant Louver - Enhanced Protection Level E | [enter]  | [enter]  | [enter]  |
| HVRR-FO | High Velocity Rain Resistant with Blades Fully Open | [enter]  | [enter]  | [enter]  |
| HVRR & IR–FO-D | High Velocity Rain Resistant with Blades Fully Open & Impact Resistant Louver - Basic Protection Level D | [enter]  | [enter]  | [enter]  |
| HVRR &IR–FO-E | High Velocity Rain Resistant with Blades Fully Open & Impact Resistant Louver - Enhanced Protection Level E | [enter]  | [enter]  | [enter]  |
| IR-B | Impact Resistant Louver - Basic Protection Level D | [enter]  | [enter]  | [enter]  |
| IR-E | Impact Resistant Louver - Enhanced Protection Level E | [enter]  | [enter]  | [enter]  |
| 410BL-CHI | Publication 410-96 - Recommended Safety Practices for Users & Installers of Industrial and Commercial Fans - Chinese | [enter]  | [enter]  | [enter]  |
| 410BL-ENG | Publication 410-96 - Recommended Safety Practices for Users & Installers of Industrial and Commercial Fans - English | [enter]  | [enter]  | [enter]  |
| **Sub-total** | [enter]  | [enter]  |
| AMCA use only: Shipping & handling |  |

We agree that AMCA Certified Rating Program seals and labels are the property of the Air Movement and Control Association (AMCA) International, Inc. Reproductions are strictly prohibited and can only be obtained through AMCA International USA headquarters. Seals and labels can only be ordered and applied to products by the licensees who have the listed product in the appendices to the License Agreement and in accordance with AMCA Publication 11-22 and AMCA Publication 512-09. Orders require payment up front, and the company must have no outstanding invoices for other AMCA resources before shipment.